# RSPPG E005 Appendices

## Appendix 1: Site Assessment Record

### The following check list is recommended for use when assessing the need for an at‑grade pedestrian crossing or changing an existing pedestrian crossing to another type. It should be completed in conjunction with a location plan (scale 1:2500) as outlined in Step 1 of this procedure guide and a general arrangement of the site at 1:500 scale.

1. **SITE CHARACTERISTICS**

|  |  |
| --- | --- |
| Site Location | DescriptionOrdnance Survey Grid Reference |
|  |  |
| Carriageway Type | Single/DoubleOne Way/Two WayNumber of Lanes |
|  |  |
| Carriageway Width |  |
|  |  |
| Footway Width | Side 1Side 2 |
|  |  |
| Refuge Island | Yes/No |
|  |  |
| Minimum Visibility | Pedestrian to vehicle Direction 1 Direction 2Vehicle to crossing Direction 1 Direction 2 |
|  |  |
| Nearby Junctions | Yes/NoDistance to nearest junction Direction 1Distance to nearest junction Direction 2 |
|  |  |
| Nearby Crossings | Yes/NoDistance to nearest controlled crossing facility Direction 1Distance to nearest controlled crossing facility Direction 2Type: Zebra/Pelican/Puffin/Toucan/Other |
|  |  |
| Waiting Restrictions | At site Yes/No TypeWithin 50 metres of site Yes/No Type |
|  |  |
| On Street Parking | Yes/No |
|  |  |
| Bus Stop | Within 50 metres of site Yes/No  |
|  |  |
| Taxi Stand | Within 50 metres of site Yes/No  |
|  |  |
| School Crossing Patrol | Yes/NoDistance from site |
|  |  |
| Local Amenities | HospitalHealth Centre/Doctor's SurgerySheltered HousingWorkshop for Disabled PeopleSchool/Nursery/Play GroupPost OfficeLeisure Facility/Play Area/Public ParkOthers including Pedestrian Leisure/Shopping AreaSports Stadium/Entertainment VenueChurch Hall/Community Centre |
|  |  |
| Pedestrian Generators | Housing developmentsBus StationRail Station |
|  |  |
| Existing Desire lines/Established Walking Routes | Yes/NoLocationDescription |